Protecto Wrap Co.

1955 South Cherokee St.

Denver, CO 80223

Phone: (800) 759-9727

Phone: (303) 777-3001

Fax: (303) 777-9273

E-mail: info@protectowrap.com

www.protectowrap.com

This MANU-SPEC utilizes the Construction Specifications Institute (CSI) Project Resource Manual (PRM), including MasterFormatTM, SectionFormatTM and PageFormatTM. A MANU-SPEC is a manufacturer-specific proprietary product specification using the proprietary method of specifying applicable to project specifications and master guide specifications. Optional text is indicated by brackets []; delete optional text in final copy of specification. Specifier Notes typically precede specification text; delete notes in final copy of specification. Trade/brand names with appropriate symbols typically are used in Specifier Notes; symbols are not used in specification text. Metric conversion, where used, is soft metric conversion.

This MANU-SPEC specifies Ice & Water Guard, a rubberized asphalt, peel-and-stick underlayment for use on sloped roofs to prevent water damage caused by ice damming. This product is manufactured by Protecto Wrap Co. Revise MANU-SPEC section number and title below to suit project requirements, specification practices and section content. Refer to CSI MasterFormatTM for other section numbers and titles.

SECTION 073000 - STEEP SLOPE ROOFING

PART 1 - GENERAL

1.1	SUMMARY

A.	Section Includes: Ice and water control underlayment.

A.	Related Sections:

1.	Roof Covering Materials: Division 07 steep slope roofing sections.

1.1	REFERENCES

A.	ASTM International:

1.	ASTM D146 Standard Test Methods for Sampling and Testing Bitumen-Saturated Felts and Woven Fabrics for Roofing and Waterproofing.

1.	ASTM D412 Standard Test Methods for Vulcanized Rubber and Thermoplastic Elastomers-Tension.

1.	ASTM D882 Standard Test Method for Tensile Properties of Thin Plastic Sheeting.

1.1	SUBMITTALS

A.	General: Submit listed submittals in accordance with Conditions of the Contract and Division 01 Submittal Procedures Section.

A.	Product Data: Submit product data for specified products.

A.	Samples: Submit 6 inch x 6 inch (152 x 152 mm) samples of specified membrane.

1.1	QUALITY ASSURANCE

A.	Regulatory Requirements and Approvals: [Specify applicable requirements of regulatory agencies.].

1.	[Code agency name].

a.	[Report or approval number].

1.1	DELIVERY, STORAGE & HANDLING

A.	General: Comply with Division 01 Product Requirements Section.

A.	Delivery: Deliver materials in manufacturer's original, unopened, undamaged containers with identification labels intact.

A.	Storage and Protection: Store materials protected from exposure to harmful environmental conditions and at temperature and humidity conditions recommended by the manufacturer.

1.1	WARRANTY

A.	Project Warranty: Refer to Conditions of the Contract for project warranty provisions.

A.	Manufacturer's Warranty: Submit, for Owner's acceptance, manufacturer's standard warranty document executed by authorized company official. Manufacturer's warranty is in addition to, and not a limitation of, other rights Owner may have under Contract Documents.

1.	Warranty Period: 5 years commencing on Date of Substantial Completion.

PART 1 - PRODUCTS

1.1	UNDERLAYMENT

A.	Manufacturer: Protecto Wrap Co.

1.	Contact: 1955 South Cherokee St., Denver, CO 80223; Telephone: (800) 759-9727, (303) 777-3001; Fax: (303) 777-9273; E-mail: info@protectowrap.com; website: www.protectowrap.com.

A.	Substitutions: No substitutions permitted.

1.1	MATERIALS

A.	Underlayment: Ice & Water Guard.

1.	Composition: Reinforced SBS modified rubberized asphalt.

1.	Thickness: 40 mils, ? 5 mils.

1.	Tensile Strength (reinforcing only): Not less than 1400 psi (9646 kPa) when tested in accordance with ASTM D882.

1.	Elongation (ultimate failure of tar mass): 500% when tested in accordance with ASTM D412.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.1	ACCESSORIES

A.	Primer: No. 100 Primer.

PART 1 - EXECUTION

1.1	MANUFACTURER'S INSTRUCTIONS

A.	Compliance: Comply with manufacturer's product data, including product technical bulletins, product catalog installation instructions and product carton instructions for installation.

1.1	EXAMINATION

A.	Site Verification of Conditions: Verify that substrate conditions, which have been previously installed under other sections, are acceptable for product installation in accordance with manufacturer's instructions.

1.1	PREPARATION

A.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

END OF SECTION