Protecto Wrap Co.

1955 South Cherokee St.

Denver, CO 80223

Phone: (800) 759-9727

Phone: (303) 777-3001

Fax: (303) 777-9273

E-mail: info@protectowrap.com

www.protectowrap.com

This MANU-SPEC utilizes the Construction Specifications Institute (CSI) Project Resource Manual (PRM), including MasterFormatTM, SectionFormatTM and PageFormatTM. A MANU-SPEC is a manufacturer-specific proprietary product specification using the proprietary method of specifying applicable to project specifications and master guide specifications. Optional text is indicated by brackets []; delete optional text in final copy of specification. Specifier Notes typically precede specification text; delete notes in final copy of specification. Trade/brand names with appropriate symbols typically are used in Specifier Notes; symbols are not used in specification text. Metric conversion, where used, is soft metric conversion.

This MANU-SPEC specifies Jiffy Seal 140/60 peel-and-stick sheet membrane waterproofing products. These products are manufactured by Protecto Wrap Co. Revise MANU-SPEC section number and title below to suit project requirements, specification practices and section content. Refer to CSI MasterFormat for other section numbers and titles.

SECTION 071300 - SHEET WATERPROOFING

PART 1 - GENERAL

1.1	SUMMARY

1.1	REFERENCES

A.	ASTM International (ASTM):

1.	ASTM D146 Standard Test Methods for Sampling and Testing Bitumen-Saturated Felts and Woven Fabrics for Roofing and Waterproofing.

1.	ASTM D412 Standard Test Methods for Vulcanized Rubber and Thermoplastic Elastomers - Tension.

1.	ASTM D570 Standard Test Method for Water Absorption of Plastics.

1.	ASTM E96 Standard Test Methods for Water Vapor Transmission of Materials.

1.	ASTM E154 Standard Test Methods for Water Vapor Retarders Used in Contact with Earth Under Concrete Slabs, on Walls, or as Ground Cover.

A.	General Services Administration, Public Building Service (GSA):

1.	PBS 07115 Guide Specification for Elastomeric Roofing.

1.1	SUBMITTALS

A.	General: Submit listed submittals in accordance with Conditions of the Contract and Division 01 Submittal Procedures Section.

A.	Product Data: Submit product data, including manufacturer's SPEC-DATA sheet, for specified products.

A.	Samples: Submit 6 inch x 6 inch (152 x 152 mm) samples of specified membrane(s).

1.1	QUALITY ASSURANCE

A.	Regulatory Requirements and Approvals: [Specify applicable requirements of regulatory agencies.].

1.	[Code agency name].

a.	[Report or approval number].

1.1	DELIVERY, STORAGE & HANDLING

A.	General: Comply with Division 01 Product Requirements Section.

A.	Delivery: Deliver materials in manufacturer's original, unopened, undamaged containers with identification labels intact.

A.	Storage and Protection: Store materials protected from exposure to harmful environmental conditions and at temperature and humidity conditions recommended by the manufacturer.

1.1	WARRANTY

A.	Project Warranty: Refer to Conditions of the Contract for project warranty provisions.

A.	Manufacturer's Warranty: Submit, for Owner'sacceptance, Manufacturer's standard warranty document executed by authorized company official. Manufacturer's warranty is in addition to, and not a limitation of, other rights Owner may have under Contract Documents.

1.	Warranty Period: 5 years commencing on Date of Substantial Completion.

PART 1 - PRODUCTS

1.1	SHEET WATERPROOFING

A.	Manufacturer: Protecto Wrap Co.

1.	Contact: 1955 South Cherokee St., Denver, CO 80223; Telephone: (800) 759-9727, (303) 777-3001; Fax: (303) 777-9273; E-mail: info@protectowrap.com; website: www.protectowrap.com.

A.	Substitutions: No substitutions permitted.

1.1	MATERIALS

A.	Jiffy Seal 140/60:

1.	Thickness: 60 mils (1.5 mm).

1.	Tensile Strength: As follows when tested in accordance with ASTM D412:

a.	Membrane: 425 psi.

a.	Polyester Reinforcement: 3200 psi.

1.	Elongation: 500% when tested in accordance with ASTM D412.

1.	Permeance: 0.003, maximum, when tested in accordance with ASTM E96, Method B.

1.	Puncture Resistance: 80 pounds (356 N) when tested in accordance with ASTM E154.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.	Tensile Strength: 600 psi (4.1 MPa), minimum, when tested in accordance with ASTM D412.

1.	Water Absorption: 0.23, maximum, when tested in accordance with ASTM D570.

1.	Exposure to Fungi in Soil (16 week exposure): Unaffected when tested in accordance with GSA PBS 07115.

A.	Jiffy Seal 140/60 CW:

1.	Thickness: 60 mils (1.5 mm).

1.	Tensile Strength: As follows when tested in accordance with ASTM D412:

a.	Membrane: 425 psi.

a.	Polyester Reinforcement: 3200 psi.

1.	Elongation: 500% when tested in accordance with ASTM D412.

1.	Permeance: 0.003, maximum, when tested in accordance with ASTM E96, Method B.

1.	Puncture Resistance: 80 pounds (356 N) when tested in accordance with ASTM E154.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.	Tensile Strength: 600 psi (4.1 MPa), minimum, when tested in accordance with ASTM D412.

1.	Water Absorption: 0.23, maximum, when tested in accordance with ASTM D570.

1.	Exposure to Fungi in Soil (16 week exposure): Unaffected when tested in accordance with GSA PBS 07115.

A.	Jiffy Seal 140/60 AK:

1.	Thickness: 60 mils (1.5 mm).

1.	Tensile Strength: As follows when tested in accordance with ASTM D412:

a.	Membrane: 425 psi.

a.	Polyester Reinforcement: 3200 psi.

1.	Elongation: 500% when tested in accordance with ASTM D412.

1.	Permeance: 0.003, maximum, when tested in accordance with ASTM E96, Method B.

1.	Puncture Resistance: 80 pounds (356 N) when tested in accordance with ASTM E154.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.	Tensile Strength: 600 psi (4.1 MPa), minimum, when tested in accordance with ASTM D412.

1.	Water Absorption: 0.23, maximum, when tested in accordance with ASTM D570.

1.	Exposure to Fungi in Soil (16 week exposure): Unaffected when tested in accordance with GSA PBS 07115.

A.	Jiffy Seal 400:

1.	Thickness: 70 mils (1.8 mm).

1.	Tensile Strength: As follows when tested in accordance with ASTM D412:

a.	Membrane: 425 psi.

a.	Polyester Reinforcement: 3200 psi.

1.	Elongation: 500% when tested in accordance with ASTM D412.

1.	Permeance: 0.002, maximum, when tested in accordance with ASTM E96, Method B.

1.	Puncture Resistance: 80 pounds (356 N) when tested in accordance with ASTM E154.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.	Tensile Strength: 500 psi (3.5 MPa), minimum, when tested in accordance with ASTM D412.

1.	Water Absorption: 0.23, maximum, when tested in accordance with ASTM D570.

1.	Exposure to Fungi in Soil (16 week exposure): Unaffected when tested in accordance with GSA PBS 07115.

A.	Jiffy Seal 500:

1.	Thickness: 60 mils (1.5 mm).

1.	Elongation: 1500% when tested in accordance with ASTM D412.

1.	Permeance: 0.003, maximum, when tested in accordance with ASTM E96, Method B.

1.	Pliability: Passes when tested in accordance with ASTM D146.

1.	Water Absorption: 0.23, maximum, when tested in accordance with ASTM D570.

1.	Exposure to Fungi in Soil (16 week exposure): Unaffected when tested in accordance with GSA PBS 07115.

1.1	ACCESSORIES

A.	Jiffy Seal No. 100 Primer.

A.	Jiffy Seal No. 100 VOC Primer.

A.	Jiffy Seal No. 80 Primer.

A.	Jiffy Seal No. 80 VOC Primer.

A.	Jiffy Seal No. 80 Green Primer.

A.	Jiffy Seal No. 6000 Water-Based Primer.

Specifier Note: Mastic below is used for sealing detail cuts and membrane terminations and should always be retained.

A.	Jiffy Seal No. JS160H Mastic.

PART 1 - EXECUTION

Specifier Note: Paragraph below is an addition to CSI SectionFormat and a supplement to MANU-SPEC. Retain or delete paragraph below per project requirements and specifier's practice.

1.1	MANUFACTURER'S INSTRUCTIONS

A.	Compliance: Comply with manufacturer's product data, including product technical bulletins, product catalog installation instructions and product carton instructions for installation.

1.1	EXAMINATION

A.	Site Verification of Conditions: Verify that substrate conditions, which have been previously installed under other sections, are acceptable for product installation in accordance with manufacturer's instructions.

1.1	PREPARATION

A.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

END OF SECTION